( TL19E00G10110249112FAAT00 )

Radiator and A/C Condenser Fan Low Speed Circuit Troubleshooting

1. Check for continuity between under-hood fuse/relay box connector B (14P) No. 11 terminal and the radiator fan 2P connector No. 1 terminal.

Is there continuity?

YES | - | Go to Step 27 .
NO | - | Repair open in the wire between the under-hood fuse/relay box and the radiator fan.■

1. Reconnect under-hood fuse/relay box connector B (14P) and the radiator fan 2P connector.

1. Disconnect the A/C condenser fan 2P connector.

1. Turn the ignition switch to ON (II), then set the A/C button and fan control button ON.