( TL19E00J34200057269KBAT00 )

Sunroof Glass Replacement

1. Remove the glass (A) by lifting it up. Do not damage the roof panel.

1. Install the glass in the reverse order of removal, then do these items:
   - Do the glass position alignment procedure.
   - Reset the sunroof control unit.

1. Check for water leaks. Use free-flowing water from a hose without a nozzle. Do not use high-pressure water.
   NOTE: It is normal for some water to seep past the sunroof into the sunroof frame, and exit through the drains.