( TL19E00J46636234525KBAT00 )

Immobilizer-Keyless Control Unit Replacement

1. Remove the driver's dashboard undercover, then remove the dashboard lower cover.

1. Remove the steering column covers.

1. Disconnect the 7P connector (A) from the immobilizer-keyless control unit (B).

1. Remove the two screws and the immobilizer-keyless control unit.

1. Install the immobilizer-keyless control unit in the reverse order of removal.

1. After replacement, register the immobilizer-keyless control unit, and make sure the immobilizer system works properly.

1. Program all of the customer's keys/keyless transmitters.