( TL19E00D14300014791MDAT20 )

Rear Brake Pad Inspection and Replacement

Replacement - Rear disc brake type

1. Remove some brake fluid from the master cylinder.

1. Raise the rear of the vehicle, and support it with safety stands in the proper locations.

1. Remove the rear wheels.

1. Remove the brake hose mounting bolt (A).

1. Remove the flange bolts (B) while holding respective caliper pin (C) with a wrench. Be careful not to damage the pin boot, and remove the caliper (D). Check the hose, the pin boots, and the parking brake cable boots for damage and deterioration.
   NOTE: Do not twist the brake hose and the parking brake cable to prevent damage.