( TL19E00J26273460309KDAT00 )

Interior Trim Removal/Installation - Trunk Lid

1. Remove the clip, then remove the trunk lid hinge trim B by detaching the hooks (A). On the right side on RHD model, release the trunk lid opener cable (C) from the hooks (D) of the trim.

1. Install the trim in the reverse order of removal, and note these items:
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Right side: Make sure the trunk lid opener cable is routed properly.
   - Push the clips and the hooks into place securely.