( TL19E00F00000057161KCAT00 )

Steering Wheel Installation

SRS components are located in this area. Review the SRS component locations, and the precautions and procedures before doing repairs or service.

1. Before installing the steering wheel, make sure the front wheels are pointing straight ahead, then center the cable reel (A). Do this by first rotating the cable reel clockwise until it stops. Then rotate it counterclockwise about three full turns. The arrow mark (B) on the cable reel label should point straight up.