( TL19E00J4616185367CKBAT00 )

Front Seat Up-down Motor Motor Replacement

Front Up-down Motor - 8-Way Power Seat
NOTE:

- Put on gloves to protect your hands.
- The driver's seat on LHD model is shown; the passenger's seat is symmetrical; the ones on RHD model are similar.

1. Remove the front seat.

1. Remove the seat cushion cover/pad.

1. Remove the front up-down motor (A) and the front up-down motor bracket (B) as an assembly:

   -1. | Disconnect the motor connector (C).
   -2. | Using a TORX T30 bit, remove the motor bracket mounting bolts (D).
   -3. | Using a TORX T40 bit, remove the motor bracket mounting bolt (E).