( TL19E20A20326400000BAAT00 )

Fuel Pressure Relieving

1. Disconnect the quick-connect fitting (A): Hold the connector (B) with one hand, and squeeze the retainer tabs (C) with the other hand to release them from the locking tabs (D). Pull the connector off.
   NOTE:
   - Be careful not to damage the line (E) or other parts.
   - Do not use tools.
   - If the connector does not move, keep the retainer tabs pressed down, and alternately pull and push the connector until it comes off easily.
   - Do not remove the retainer from the line; once removed, the retainer must be replaced with a new one.

1. After disconnecting the quick-connect fitting, check it for dirt or damage.

1. Do the battery terminal reconnection procedure.