( TL19E00J26216516401KDAT00 )

Center Console Removal/Installation

1. Remove the center console (A). LHD model is shown; RHD model is symmetrical.

   -1. | Detach the clips (B, C, D) by pulling the front edges of the center console out from both sides.
   -2. | Pull up the console to release the hooks (E).
   -3. | With rear ventilation: Pull the console rearward to disconnect both the side ducts (F).

Without rear ventilation
With rear ventilation