( TL19E00H10800000000FAAT00 )

ACC Troubleshooting

1. Check the No. 2 (7.5 A) fuse in the driver's under-dash fuse/relay box.

Is the fuse OK?

YES | - | Go to Step 2 .
NO | - | Check for a short in the wire between the No. 2 (7.5 A) fuse socket and the ACC unit. If OK, replace the fuse.■

1. Disconnect the 20P connector from the ACC unit.

1. Turn the ignition switch to ON (II).

1. Check for voltage between the ACC unit 20P connector No. 2 terminal and body ground.

Is there battery voltage?

YES | - | Go to Step 5 .
NO | - | Repair an open in the wire between the No. 2 (7.5 A) fuse in the driver's under-dash fuse/relay box and the ACC unit. If the wire is OK, replace the driver's under-dash fuse/relay box.■

1. Turn the ignition switch to LOCK (0).