( TL19E00D52100063635KDAT00 )

VSA Modulator-control Unit Removal and Installation

Installation

1. Install the VSA modulator-control unit onto the bracket.

1. Install the clips to the bracket, then install the receiver line.

1. Install the bracket with the VSA modulator-control unit to the body.

1. Reconnect the six brake lines, then tighten the flare nuts to the specified torque.

1. Align the connecting surface of the VSA modulator-control unit 47P connector to the VSA modulator-control unit.

1. Pull up the lever of the VSA modulator-control unit 47P connector, then confirm the connector is fully seated.

1. Install the suction line mount bolt to the bracket.

1. Bleed the brake system.

1. Do the VSA sensor neutral position memorization procedure.

1. Start the engine, and check that the ABS and the VSA indicators go off.

1. Test-drive the vehicle, and make sure that the ABS and the VSA indicators do not come on.
   NOTE: If the brake pedal is spongy, there may be air trapped in the modulator which could then be induced into the normal brake system during modulation. Bleed the brake system again.