( TL19E00E16236500000KCAT00 )

Intermediate Shaft Installation

1. Clean the areas where the intermediate shaft contacts the differential thoroughly with solvent or brake cleaner, and dry with compressed air.
   NOTE: Do not wash the rubber parts with solvent.

1. Install a new set ring (A) onto the set ring groove (B) of the intermediate shaft (C).
   NOTE: The illustrations show K24Z3 engine model.

1. Insert the intermediate shaft into the differential correctly.
   NOTE: Insert the intermediate shaft carefully to prevent damaging the oil seal (D).