( TL19E00H46400012802KBAT00 )

Driver's Airbag Replacement

1. Connect the driver's airbag 4P connector (A) to the cable reel 4P connector, then install the access panel (B) on the steering wheel.

1. Do the battery terminal reconnection procedure.

1. Connect the HDS, and clear the DTCs.

1. After installing the airbag, confirm proper system operation:
   - Turn the ignition switch to ON (II); the SRS indicator should come on for about 6 seconds and then go off.
   - Make sure the horn works.