( TL19E00B20200036401KBAT00 )

Front Knuckle/Hub/Wheel Bearing Replacement

1. Check the front knuckle ring (A) for damage or deformation, and replace it if necessary.
   NOTE: When installing the new front knuckle ring, position the knuckle ring notch portion (B) toward cut out (C) near the ball joint in the knuckle, and align the center of the knuckle ring ledge portion (D) with the center of the wheel sensor hole (E) on the knuckle as shown.