( TL19E20A20326428521KDAT00 )

Fuel Tank Unit Removal and Installation

1. Using the special tool, tighten a new locknut (A) with a new locknut plate (B) to the specified torque.
   NOTE:
   - Before tightening, align the marks (C) on the fuel tank and locknut.
   - After tightening, make sure the marks are still aligned.
   - After installation, check the base gasket, visually or by hand, to make sure it is not pinched.

1. Connect the fuel tank unit 4P connector, then connect the quick-connect fitting.

1. Reconnect the negative cable to the battery, and turn the ignition switch to ON (II) (but do not operate the starter motor). The fuel pump will run for about 2 seconds, and fuel pressure rises. Repeat this two or three times, then check that there is no leakage in the fuel supply system.

1. Install the access panel.

1. Install the rear seat cushion.