( TL19E1RE10436455079KBAT00 )

A/T Interlock System - Shift Lock Release, Release Spring, and Release Extension Replacement

1. Install the shift lock release (A) while aligning the tab (B) with the tab slot (C), while hooking the release spring end (D) in the slot (E), and set the stop lever (F) on the stop (G).

1. Install the shift lock release extension (H).

1. Install the shift lever boot and the A/T gear position indicator panel base.

1. Install the shift lever knob.

1. Install the shift lever assembly.