( TL19E00D14300014791MDAT20 )

Rear Brake Pad Inspection and Replacement

Replacement - Rear drum in disc brake type

1. Remove some brake fluid from the master cylinder.

1. Raise the rear of the vehicle, and support it with safety stands in the proper locations.

1. Remove the rear wheels.

1. Remove the flange bolts (A) while holding respective caliper pin (B) with a wrench. Be careful not to damage the pin boot, and remove the caliper (C). Check the hose and the pin boots for damage and deterioration.
   NOTE: Do not twist the brake hose to prevent damage.