( TL19E00J4616645402QKBAT00 )

Rear Seat Release Lever Replacement

NOTE:

- Take care not to bend or scratch the interior trim.
- The left seat-back release lever is shown; the right seat-back release lever is similar.

1. From the trunk compartment, remove the clips, and release the hook (A), then remove the seat-back release lever (B).
   NOTE: To remove the clips, pry the inner clip up at the edge near the line (C) on its head.

1. Disconnect the rear seat-back release cable (A). Take care not to kink the cable.

1. Install the release lever in the reverse order of removal, and note these items:
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Make sure the release cable is connected securely.
   - Make sure the seat-back locks securely and unlocks properly.