( TL19E00H46400056801KBAT00 )

SRS Unit Replacement

Removal

1. Do the battery terminal disconnection procedure, then wait for 3 minutes before starting work.

1. Remove the driver's dashboard lower cover and passenger's dashboard lower cover.

1. Using a TORX T30 bit, remove the TORX bolt (A).

1. With navigation: Remove the audio unit.

1. Without navigation: Remove the dashboard center pocket.

1. Disconnect SRS unit connector A (39P) and connector B (39P), and remove the TORX bolts (C) using a TORX T30 bit, then pull out the SRS unit.

Installation

1. Install the SRS unit (A) with a new TORX bolt (B), using a TORX T30 bit.
   NOTE: Be sure the SRS unit is sitting squarely against it's bracket before torquing the TORX bolt.

1. Using a TORX T30 bit, install the new TORX bolts (A), then connect the connectors (B) to the SRS unit; push them into position until they click.

1. Do the battery terminal reconnection procedure.

1. Confirm proper SRS operation: Turn the ignition switch ON (II); the SRS indicator should come on for about 6 seconds and then go off.

1. Reinstall all removed parts.