( TL19E00H32500036861MBAT00 )

LKAS Camera Aiming

1. Move the camera aimer set, and make a target pattern central point agree with floor surface position Y1 of the right side.
   NOTE: To make the adjustment correctly, align the plumbs so that each of them attached with tip of the plumb bob on a string.

1. Check ‘‘the right side target detection'' from the HDS.

1. Check ‘‘the right side target detection'' was successful on the HDS.
   NOTE: If the aiming has failed or is aborted, you must start the static camera aiming procedure again.