( TL19E00H46400000000CAAT00 )

SRS Unit Inputs and Outputs at Connector A (39P)

Terminal Number | Wire Color | Terminal Name | Description
--- | --- | --- | ---
3 | BRN * | LA1− | Ground for the driver's airbag first inflator (LHD model)
Ground for the passenger's airbag first inflator (RHD model)
4 | LT BLU * | LA1+ | Power source for the driver's airbag first inflator (LHD model)
Power source for the passenger's airbag first inflator (RHD model)
5 | BLU * | RA1− | Ground for the passenger's airbag first inflator (LHD model)
Ground for the driver's airbag first inflator (RHD model)
6 | YEL * | RA1+ | Power source for the passenger's airbag first inflator (LHD model)
Power source for the driver's airbag first inflator (RHD model)
16 | RED * | CAN LO | Sends and receives communication signal from the gauge control module
17 | WHT * | CAN HI | Sends and receives communication signal from the gauge control module
18 | LT BLU * | K-LINE | Sends and receives scan tool signal (serial data)
20 | BLU | PTT | Sends and receives communication signal with the passenger's airbag off indicator
21 | BLU | ACS | Power source for the front passenger's airbag ON/OFF switch
26 | YEL * | VA | SRS system sub power (common with OPDS)
27 | RED * | VB | SRS dedicated power (dedicated booster circuit)
28 | BLK * | SRS GND 1 | Ground circuit for the SRS unit (G504)
29 | BLK * | SRS GND 2 | Ground circuit for the SRS unit (G504)
31 | RED * | WEN | Data link connector
36 | BRN * | LFS− | Ground for the left front impact sensor
37 | RED * | LFS+ | Power source for the left front impact sensor
38 | LT BLU * | RFS− | Ground for the right front impact sensor
39 | GRN * | RFS+ | Power source for the right front impact sensor

*: | Wire colors may be substituted in this table.