( TL19E00J1616622130AKBAT00 )

Rear Door Outer Molding Replacement

NOTE:

- If you remove the door outer molding, replace it with a new one because it will bend during removal.
- Put on gloves to protect your hands.
- Take care not to scratch the door.
- When removing components, use the trim tools or equivalent.

1. Remove these items:
   - Door panel
   - Door panel bracket
   - Plastic cover, as needed
   - Door glass outer weatherstrip

1. Using a clip remover, detach the clips (A), then pull back the door weatherstrip (B), and remove the screws (C, D).