( TL19E00J18573560341KBAT00 )

Trunk Lid Torsion Bar Replacement

1. Install the torsion bars in the reverse order of removal, and note these items:
   - The shapes of the right torsion bar (A) and the left torsion bar (B) are shown. Install the torsion bars properly.
   - Adjust the torsion bars forward or rearward with the torsion bar assembly tool.
   - Positions where each torsion bar was installed in the factory are following:

   - | Left torsion bar: Normal position
   - | Right torsion bar: Normal position

   - Make sure the trunk lid opens properly and locks securely.