( TL19E30A14100012901KDAT00 )

Alternator Removal and Installation

Removal

1. Do the battery terminal disconnection procedure.

1. Remove the drive belt.

1. Remove the two bolts securing the alternator.

1. Disconnect the alternator connector (A), BLK wire (B), and harness clamp (C) from the alternator, then remove the alternator.

Installation

1. Connector the alternator connector (A), BLK wire (B), and harness clamp (C) to the alternator. Make sure the crimped it side of the ring terminal faces away form the alternator when you connect it.

1. Tighten the two bolts securing the alternator.

1. Install the drive belt.

1. Do the battery terminal reconnection procedure.