( TL19E1PE10410600000CAAT00 )

Electronic Control System (cont'd)
PCM A/T Control System Inputs and Outputs - R20A3 Engine Model (cont'd)
PCM CONNECTOR C ○ (44P)

Terminal Number | Wire Color | Terminal Name | Description | Signal
--- | --- | --- | --- | ---
C13 | YEL/RED | VCC1 (SENSOR VOLTAGE) | Provides sensor voltage | With ignition switch ON (II): About 5.0 V With ignition switch LOCK (0): About 0 V
C14 | GRN/WHT | SG1 (SENSOR GROUND) | Sensor ground | Less than 0.5 V at all times
C36 | BLK/YEL | IG1 (IGNITION SIGNAL) | Detects ignition switch signal | With ignition switch ON (II): Battery voltage With ignition switch LOCK (0): About 0 V
C40 | BRN/YEL | LG1 (LOGIC GROUND) | Ground circuit for PCM | Less than 0.5 V at all times
C43 | BLK/WHT | NC (OUTPUT SHAFT (COUNTERSHAFT) SPEED SENSOR) | Detects output shaft (countershaft) speed sensor signal | With ignition switch ON (II): About 0 V or about 5.0 V With driving: About 2.5 V (pulses)
C44 | BRN/YEL | LG2 (LOGIC GROUND) | Ground circuit for PCM | Less than 0.5 V at all times

PCM A/T Control System Electrical Connections - K24Z3 Engine Model