( TL19E20A20326428001KCAT00 )

Fuel Line/Quick-Connect Fitting Installation

1. Align the quick-connect fittings with the line (A), and align the retainer locking tabs (B) with the connector grooves (C). Then press the quick-connect fittings onto the line until both retainer tabs lock with a clicking sound.
   NOTE: If it is hard to connect, put a small amount of new engine oil on the line end.

Connection with new retainer
Connection to new fuel line
Reconnection to existing retainer