( TL19E20A20326428302FAAT00 )

Fuel Pump Circuit Troubleshooting

1. Measure the voltage between PGM-FI main relay 2 4P connector terminal No. 2 and body ground.

Is there battery voltage?

YES | - | Replace the inertia switch. ■

NO

-

- Replace the No. 9 FUEL PUMP (20 A) fuse in the driver's under-dash fuse/relay box.■
- Replace the driver's under-dash fuse/relay box. ■
- Repair open in wires between inertia switch and driver's under-dash fuse/relay box.■