( TL19E00K791000R611XFAAT01 )

DTC Troubleshooting: 61-1x - With Seat Heater

1. Measure the resistance between the No. 1 terminal of the Driver′s (LHD model) or passenger′s (RHD model) seat wire harness 2P connector and body ground. There should be 0−1.0 Ω.

Is resistance as specified?

YES | - | Faulty left side seat belt buckle switch; replace the left side seat belt buckle assembly. ■
NO | - | Open in the driver's (LHD model) or passenger's (RHD model) seat wire harness, SRS floor wire harness; replace the faulty harness.■