( TL19E00J54200034401FEAT00 )

Ignition Switch Test

SRS components are located in this area. Review the SRS component locations and precautions and procedures before performing repairs or servicing.

1. Do the battery terminal disconnection procedure.

1. Remove the steering column covers.

1. Disconnect the 5P connector (A) from the ignition switch (B).

1. Check for continuity between the terminals in each switch position according to the table.

1. If the continuity does not agree with the table, replace the ignition switch.

1. Do the battery terminal reconnection procedure.