( TL19E20A20326427702FEAT00 )

Fuel Gauge Sending Unit Test

1. Measure the voltage between fuel tank unit 4P connector terminals No. 1 and No. 3 with the ignition switch to ON (II). There should be battery voltage.
   - If the voltage is OK, go to Step 8 .
   - If the voltage is not as specified, check for:

   - | a short in the PUR wire to ground.
   - | an open in the PUR or ORN wire.

1. Turn the ignition switch to LOCK (0).

1. Remove the fuel tank unit from the fuel tank.