( TL19E00H46400000000CAAT00 )

SRS Unit Inputs and Outputs at Connector B (39P)
RHD model

Terminal Number | Wire Color | Terminal Name | Description
--- | --- | --- | ---
1 | ORN * | ODS | Sends and receives communication signal with the OPDS unit
4 | RED * | RLP− | Ground for the left side outer lap tensioner
5 | WHT * | RLP+ | Power source for the right side outer lap tensioner
6 | LT BLU * | LSA− | Ground for the left side airbag inflator
7 | YEL * | LSA+ | Power source for the left side airbag inflator
8 | GRN * | RSA− | Ground for the right side airbag inflator
9 | PUR * | RSA+ | Power source for the right side airbag inflator
10 | BLU * | LCA1− | Ground for the left side curtain airbag inflator
11 | BRN * | LCA1+ | Power source for the left side curtain airbag inflator
12 | WHT * | LRP− | Ground for the left side seat belt tensioner
13 | BLU * | LRP+ | Power source for the left side seat belt tensioner
14 | GRY * | RRP− | Ground for the right side seat belt tensioner
15 | PNK * | RRP+ | Power source for the right side seat belt tensioner
16 | LT GRN * | RLBC | Rear left seat belt buckle switch
17 | WHT * | RCBC | Rear center seat belt buckle switch
18 | BLU * | RRBC | Rear right seat belt buckle switch
19 | PNK * | FLBC | Left side seat belt buckle switch
21 | WHT * | FRBC | Right side seat belt buckle switch
23 | YEL * | SS+ | Front passenger's seat sitting switch
24 | RED * | RCA1− | Ground for the right side curtain airbag inflator
25 | GRN * | RCA1+ | Power source for the right side curtain airbag inflator
36 | BRN * | LBS1− | Ground for the left side impact sensor (first)
37 | GRY * | LBS1+ | Power source for the left side impact sensor (first)
38 | ORN * | RBS1− | Ground for the right side impact sensor (first)
39 | BLU * | RBS1+ | Power source for the right side impact sensor (first)

*: | Wire colors may be substituted in this table.