( TL19E2AK7210009250AFAAT00 )

DTC Troubleshooting: P250A

DTC P250A:
Engine Oil Level Sensor Circuit Malfunction
NOTE: Before you troubleshoot, record all freeze data and any on-board snapshot, and review the general troubleshooting information.

1. Turn the ignition switch to ON (II).

1. Clear the DTC with the HDS.

1. Wait 5 seconds.

1. Check for Temporary DTCs or DTCs with the HDS.

Is DTC P250A indicated?

YES | - | Go to Step 5 .
NO | - | Intermittent failure, the system is OK at this time. Check for poor connections or loose terminals at the engine oil level sensor and the ECM/PCM.■

1. Turn the ignition switch to LOCK (0).

1. Disconnect the engine oil level sensor 3P connector.

1. Turn the ignition switch to ON (II).

1. Measure the voltage between engine oil level sensor 3P connector terminal No. 3 and body ground.

Is there battery voltage?

YES | - | Go to Step 9 .
NO | - | Repair open in the wire between the engine oil level sensor and the No. 21 OIL LVL (7.5 A) fuse then go to Step 19 .

1. Check for continuity between engine oil level sensor 3P connector terminal No. 2 and body ground.

Is there continuity?

YES | - | Go to Step 10 .
NO | - | Repair open in the wire between the engine oil level sensor and G101; A/T, M/T, then go to Step 19 .

1. Measure the voltage between engine oil level sensor 3P connector terminal No. 1 and body ground.

Is there battery voltage?

YES | - | Go to Step 17 .
NO | - | Go to Step 11 .

1. Turn the ignition switch to LOCK (0).

1. Jump the SCS line with the HDS.

1. Disconnect ECM/PCM connector C (44P).

1. Check for continuity between ECM/PCM connector terminal C37 and body ground.

Is there continuity?

YES | - | Repair short in the wire between the ECM/PCM (C37) and the engine oil level sensor, then go to Step 19 .
NO | - | Go to Step 15 .

1. Connect engine oil level sensor 3P connector terminal No. 1 to body ground with a jumper wire.

1. Check for continuity between ECM/PCM connector terminal C37 and body ground.

Is there continuity?

YES | - | Go to Step 24 .
NO | - | Repair open in the wire between the ECM/PCM (C37) and the engine oil level sensor, then go to Step 19 .

1. Turn the ignition switch to LOCK (0).

1. Replace the engine oil level sensor.

1. Reconnect all connectors.

1. Turn the ignition switch to ON (II).

1. Reset the ECM/PCM with the HDS.

1. Do the ECM/PCM idle learn procedure.

1. Check for Temporary DTCs or DTCs with the HDS.

Is DTC P250A indicated?

YES | - | Check for poor connections or loose terminals at the engine oil level sensor and the ECM/PCM, then go to Step 1 .
NO | - | Troubleshooting is complete. If any other Temporary DTCs or DTCs are indicated, go to the indicated DTC's troubleshooting.■

1. Reconnect all connectors.

1. Update the ECM/PCM if it does not have the latest software, or substitute a known-good ECM/PCM.

1. Check for Temporary DTCs or DTCs with the HDS.

Is DTC P250A indicated?

YES | - | Check for poor connections or loose terminals at the engine oil level sensor and the ECM/PCM. If the ECM/PCM was updated, substitute a known-good ECM/PCM, then recheck. If the ECM/PCM was substituted, go to Step 1 .
NO | - | If the ECM/PCM was updated, troubleshooting is complete. If the ECM/PCM was substituted, replace the original ECM/PCM. If any other Temporary DTCs or DTCs are indicated, go to the indicated DTC's troubleshooting.■