( TL19E00J00061545171KBAT00 )

Parking and Back-up Sensor Control Unit Replacement

1. Remove the driver's dashboard undercover, then remove the dashboard lower cover.

1. Remove the bolt (A) from the bracket (B), then disconnect the 16P connector (C) from the parking and back-up sensor control unit (D). For LHD model, disconnect the 16P connector (E) from the headlight leveling control unit (F).

1. Install the parts in the reverse order of removal.

1. For LHD model, after replacement, do the headlight initial positioning learning.