( TL19E1PE10410459801KAAT00 )

A/T Housing and Shaft Assembly Removal

Special Tools Required
Housing puller
07HAC-PK40102

1. Remove the ATF feed pipe (A) from the idler gear shaft,idler gear assembly, and remove the ATF lubrication pipe (B) from the transmission housing.

1. Remove the shift solenoid valve cover (C), the dowel pins (D), and the gasket (E).

1. Disconnect the connectors from the shift solenoid valves, and remove the shift solenoid wire harness (F), then remove the O-ring (G).

1. Remove the input shaft (mainshaft) speed sensor (H), then remove the O-ring (J).

1. Remove the output shaft (countershaft) speed sensor (I) and the speed sensor washer (K) (only for K24Z3 engine model), then remove the O-ring (J).

1. Remove the transmission housing mounting bolts (19 bolts) (L) and the transmission hanger (M).