( TL19E00J16166220801KBAT00 )

Rear Door Latch Replacement

NOTE:

- Put on gloves to protect your hands.
- The latch without super locking is shown; the latch with super locking is similar.

1. Remove these items:
   - Door panel
   - Inner handle
   - Door end trim

1. Raise the glass fully.

1. Remove the plastic cover as needed.

1. Detach the rod fastener, and disconnect the outer handle rod from the outer handle base.

1. Remove the screws (A, B) securing the latch (C), then remove latch through the hole in the door. Take care not to bend the outer handle rod (D), the latch cable (E), and the inner handle cable (F).