( TL19E20A14616716091KDAT00 )

CMP Pulse Plate Removal and Installation

Removal

1. Remove the intake air duct.

1. Remove the engine mount control solenoid valve mounting bolt.

1. Remove the harness holder (A) from the cylinder head.

1. Remove the rocker arm assembly.

1. Remove the camshaft thrust cover.

1. Hold the camshaft with an open-end wrench, then loosen the bolt.

1. Remove the camshaft position (CMP) pulse plate.

Installation

1. Install the CMP pulse plate.

1. Hold the camshaft with an open-end wrench, then tighten the bolt.

   Specified Torque
   14 x 1.5 mm 34 N·m (3.5 kgf·m, 25 lbf·ft)

1. Install the camshaft thrust cover (A), use a new O-ring (B).

1. Install the rocker arm assembly.

1. Install the harness holder (A) on the cylinder head.

1. Install the engine mount control solenoid valve mounting bolt.

1. Install the intake air duct.