( TL19E20A14680200000KCAT00 )

Cylinder Head Valve, Spring, and Valve Seal Installation

Special Tools Required
Stem seal driver
07PAD-0010000
Valve spring compressor
07757-0010000

1. Coat the valve stems with new engine oil. Install the valves in the valve guides.

1. Check that the valves move up and down smoothly.

1. Install the spring seats on the cylinder head.

1. Install the new valve seals (A) using the stem seal driver (B).
   NOTE: Exhaust valve seals (C) have a black spring (D), and intake valve seals (E) have a white spring (F); they are not interchangeable.

1. Install the valve spring and the spring retainer. Place the end of the valve spring with the closely wound coils toward the cylinder head.

1. Install the valve spring compressor. Compress the spring, and install the valve cotters.

1. Remove the valve spring compressor.

1. Lightly tap the end of each valve stem two or three times with a plastic mallet (A) to ensure proper seating of the valve and the valve cotters. Tap the valve stem only along its axis so you do not bend the stem.