( TL19E00J36100000000CAAT20 )

Rearview Camera Inputs and Outputs
Rearview Camera 6P Connector

Terminal Number | Wire Color | Terminal Name | Description | Voltage (about) | Symptom
--- | --- | --- | --- | --- | ---
1 | WHT | CAMERA VCC (VCC supply) | Power source for rearview camera | 8 V | If open: No rearview camera image. If short to ground: When put into reverse, navigation screen goes black (display backlight still operative).
2 | RED | RC GND (Ground camera) | Ground for camera signal | 0 V | If open: No change to rearview camera image. If short to ground: No change to rearview camera image.
3 | GRN | CAMERA GND (Ground camera) | Ground for rearview camera | 0 V | If open: No change to rearview camera image. If short to ground: No change to rearview camera image.
4 | BLK | VIDEO (Video camera) | Video signal for rearview camera | 0.3 V | If open: No change to rearview camera image. If short to ground: No change to rearview camera image.
5 | GRY | CAMERA SH (Shield camera) | Shield for terminals No. 1, 2, 3, 4 | 0 V | If open: No change to rearview camera image. If short to ground: No change to rearview camera image.
6 | BRN | CAMERA ADPT (Adaptive camera) | Control signal for rearview camera | 0 V | If open: No change to rearview camera image. If short to ground: No change to rearview camera image.