( TL19E00K791000R421XFAAT00 )

DTC Troubleshooting: 42-1x

1. Measure the resistance between the No. 38 and the No. 39 terminals of SRS unit connector A (39P). There should be less than 1 Ω.

Is the resistance as specified?

YES | - | Faulty right front impact sensor or SRS unit; replace the right front impact sensor. If the problem is still present, replace the SRS unit. ■
NO | - | Open in the right engine compartment wire harness or dashboard wire harness; replace the faulty harness.■