( TL19E00J54400065501KBAT00 )

Windshield Replacement

1. Attach the rubber dam A, the upper clips (B), and the dashboard seals (C) with adhesive tape to the inside face of the windshield (D) as shown. Before installing the upper clips, apply primer to the area where the adhesive tape will be applied to the inside face of the windshield:
   - Be sure the rubber dam, the upper clips, and the dashboard seals line up with the alignment marks (E).
   - Be sure the convex portion (F) of the left and right clips toward right.
   - Be careful not to touch the windshield where adhesive will be applied.

   Rubber dam adhesive tape:
   | Thickness 0.16 mm (0.006 in.)
   | Width 3.5 mm (0.14 in.)
   Upper clip adhesive tape:
   | Thickness 0.4 mm (0.016 in.)
   | Width 10 mm (0.39 in.)
   Dashboard seal adhesive tape:
   | Thickness 0.4 mm (0.016 in.)
   | Width 13 mm (0.51 in.)