( TL19E1AE34116317041KBAT00 )

Clutch Pedal Assembly Replacement

1. Install the clutch pedal assembly (A).

1. Install the clutch pedal mounting bolt (B) and master cylinder mounting nuts (C).

1. Apply multipurpose grease to the pedal pin (D), and mating surfaces (E) of the yoke and the pedal. Slide it into the yoke, then install a lock pin (F).

1. Adjust the clutch pedal, clutch pedal position switch, and clutch switch (SIL).

1. Check the clutch operation.

1. Install the driver's dashboard undercover.