( TL19E2PE10400013012KBAT00 )

ATF Cooler Hose Replacement

R20A3 Engine Model

1. Slide the ATF cooler/filter hoses (A) on the ATF filter (B) until they touch the filter housing, and secure the hoses with the clips (C) at 6−8 mm (0.24−0.31 in.) (D) from the filter housing.

1. Slide the ATF cooler hoses (E) over the ATF lines (F) until the hose ends contact the bulge (G), and secure the hoses with the clips (H) at 6−8 mm (0.24−0.31 in.) (I) from the hose end.

1. Slide the ATF cooler hose (J) over the ATF cooler line (K) until the hose end contacts the bulge (L), and secure the hose with the clip (M) at 2−4 mm (0.08−0.16 in.) (N) from the hose end.

1. Slide the ATF cooler hose (O) over the ATF cooler line (P) until the hose end contacts the mark (Q), and secure the hose with the clip (R) at 2−4 mm (0.08−0.16 in.) (S) from the hose end.