( TL19E00J26273413801KDAT00 )

Interior Trim Removal/Installation - Pillar Areas

Center Pillar Upper/Lower Trim
SRS components are located in this area. Review the SRS component locations and the precautions and procedures before doing repairs or service.
NOTE:

- Put on gloves to protect your hands.
- Take care not to bend or scratch the trim and the panels.
- When removing components, use the trim tools or equivalent.

1. Remove these items:
   - Front door sill trim
   - Rear door sill trim
   - Front door opening seal, as needed
   - Rear door opening seal, as needed

1. Slide the front seat forward fully.

1. Remove the center pillar lower trim (A).

   -1. | While releasing the upper tabs (B), pull the upper portion of the trim back to detach the upper hooks (C).
   -2. | Detach the lower clips by pulling the bottom of the trim back by hand.

1. Driver's side: Unbuckle the front seat belt anchor connector.

1. Passenger's side: Remove the front seat belt lower anchor from the body.