( TL19E2AK72100090134FAAT00 )

DTC Troubleshooting: P0134 (41)

DTC P0134:
A/F Sensor (Sensor 1) Heater System Malfunction
NOTE:

- Before you troubleshoot, record all freeze data and any on-board snapshot, and review the general troubleshooting information.
- If the vehicle was out of fuel and the engine stalled before this DTC was stored, refuel and clear the DTC with the HDS.
- If DTC P0135 is stored at the same time as DTC P0134, troubleshoot DTC P0135 first, then recheck for DTC P0134.

1. Turn the ignition switch to ON (II).

1. Clear the DTC with the HDS.

1. Start the engine, and let it idle without load (A/T in P or N, M/T in neutral) until the radiator fan comes on.

1. Check for Temporary DTCs or DTCs with the HDS.

Is DTC P0134 indicated?

YES | - | Go to Step 5 .
NO | - | Intermittent failure, the system is OK at this time. Check for poor connections or loose terminals at the A/F sensor (Sensor 1), the under-hood fuse/relay box, and the ECM/PCM.■

1. Turn the ignition switch to LOCK (0).

1. Replace the A/F sensor (Sensor 1).

1. Turn the ignition switch to ON (II).

1. Reset the ECM/PCM with the HDS.

1. Do the ECM/PCM idle learn procedure.

1. Check for Temporary DTCs or DTCs with the HDS.

Is DTC P0134 indicated?

YES | - | Check for poor connections or loose terminals at the A/F sensor (Sensor 1), the under-hood fuse/relay box, and the ECM/PCM, then go to Step 1 .
NO | - | Go to Step 11 .

1. Monitor the OBD STATUS for DTC P0134 in the DTCs MENU with the HDS.

Does the screen indicate PASSED?

YES | - | Troubleshooting is complete. If any other Temporary DTCs or DTCs were indicated in Step 10 , go to the indicated DTC's troubleshooting.■
NO | - | If the screen indicates FAILED, check for poor connections or loose terminals at the A/F sensor (Sensor 1) and the ECM/PCM, then go to Step 1 . If the screen indicates NOT COMPLETED, go to Step 8 .