( TL19E00H46400000000FAAT09 )

SRS Symptom Troubleshooting - Faulty front seat belt reminder light

1. Disconnect the front passenger's seat wire harness or SRS floor wire harness 2P connector (A) from the front passenger's seat sitting switch.

1. Install a jumper wire between the No. 1 terminal and the No. 2 terminal of the front passenger's seat wire harness or SRS floor wire harness 2P connector.

1. From the Main Menu on the HDS, select SRS, then PARAMETER INFORMATION. In the PARAMETER INFORMATION Menu, select ‘‘SRS PSS'', and read the HDS indicated.

Is ON indicated on the HDS?

YES | - | Faulty front passenger's seat sitting switch; replace the seat cushion.
NO | - | Open in the front passenger's seat wire harness or SRS floor wire harness; replace the faulty wire harness.■