( TL19E00J18573455601KBAT00 )

Side Sill Panel Replacement

For Some Models
NOTE:

- Put on gloves to protect your hands.
- Take care not to scratch the body.

1. Remove the side sill panel (A).

   -1. | On the back of the front wheel arch, remove the screws (B).
   -2. | Remove the expansion clips (C).
   -3. | Slide the side sill panel forward and remove it. The side clips (D, E, F) will stay in the body.
   -4. | Remove the side clip (D) by turning the clip 45 ° from the body.
   -5. | Remove the side clip (E) from the body.
   -6. | Remove the side clip (F) by releasing the double-sided adhesive tape (G) from the body.

1. Scrape off the remaining double-sided adhesive tape from the front portion of the rear wheel arch, and clean the body surface with isopropyl alcohol.

1. If the side clips are damaged or stress-whitened, replace them with new ones.