( TL19E00K75100081050FAAT00 )

DTC Troubleshooting: 5

1. Check for continuity between LKAS control unit 26P connector No. 8 terminal and EPS control unit connector D (28P) No. 20 terminal.

Is there continuity?

YES | - | Go to Step 19 .
NO | - | Repair an open in the wire between the LKAS control unit and the EPS control unit.■

1. Check for EPS control unit DTCs with HDS.

Are any DTCs indicated?

YES | - | Troubleshoot the EPS control unit DTC(s).■
NO | - | Check for loose terminals in the EPS control unit connectors, and repair if necessary. If all connections are OK, replace the EPS control unit. ■