( TL19E00000000000000JCAT31 )

Maintenance Schedule for Normal Conditions - South Africa
75,000miles(8year)

Follow the normal conditions maintenance schedule if the severe driving conditions specified in the severe conditions maintenance schedule do not apply.
Service at the indicated distance or time whichever comes first

| Replace engine oil R20A3, K24Z3

| Replace engine oil filter R20A3, K24Z3

| Check parking brake adjustment

Check the parking brake operation.

| Tie-rod ends, steering gearbox, and boots

|  | Check rack grease and steering linkage.
|  | Check the boot for damage and leaking grease.

| Suspension components

|  | Check the bolts for tightness.
|  | Check all dust cover for deterioration and damage.

| Driveshaft boots

|  | Check the boot and boot band for cracks.
|  | Check rack grease.

| Brake hoses and lines (including VSA lines)

Check the master cylinder and VSA modulator-control unit and leakage.

| All fluid levels and condition of fluids

Check levels and check for leaks. If necessary, add.

|  | Engine coolant R20A3, K24Z3
|  | MTF
|  | ATF
|  | Brake fluid
|  | Clutch fluid
|  | Windshield washer fluid

| Exhaust system

R20A3, K24Z3
Check the exhaust pipe and muffler for damage, leaks, and tightness.

| Fuel lines R20A3, K24Z3

and connections R20A3, K24Z3

|  | Check fuel lines for loose connections, cracks, and deterioration.
|  | Retighten loose connections and replace any damaged parts.

Every 15,000 km

| Replace air cleaner element R20A3, K24Z3

| Rotate tyres

Check tyre inflation and condition at least once per month.

Every 45,000 km

| Inspect valve clearance R20A3, K24Z3

Every 105,000 km

| Replace spark plugs R20A3, K24Z3

At 200,000 km or 10 years, then every 100,000 km or 5 years

| Replace engine coolant R20A3, K24Z3

Use genuine Honda All Season Antifreeze/Coolant Type 2.

Every 10,000 km or 6 months

| Check front and rear brakes

|  | Check the brake pad and disc thickness. Check for damage or cracks.
|  | Check the calipers for damage, leaks, and tightness.

Every 3 years

| Replace brake fluid

|  | Use only DOT 3 or DOT 4 brake fluid. We recommend genuine Honda Brake Fluid.
|  | Check that brake fluid level between upper and lower marks on the reservoir.

Every 30,000 km or 1 year

| Replace dust and pollen filter

|  | If the vehicle is drive mostly in areas that have high concentrations of dust, pollen, or soot in the air, replace every 15,000 km or 1 year.
|  | Replace the filter whenever airflow from the heating and air conditioning system is less than normal.