( TL19E1AE34116317081KBAT00 )

Clutch Slave Cylinder Replacement

1. Apply a light of molybdenum grease to the pushrod (A) of the slave cylinder.

1. Connect the clutch line (B) to the slave cylinder (C), and loosely tighten the flare nut (D).

1. Install the slave cylinder to the transmission housing, then tighten the clutch line flare nut to the specified torque.
   NOTE: Tighten the flare nut while holding the clutch line connector (E) with a wrench.

1. Bleed the clutch hydraulic system.

1. Check the clutch operation, and check for leaks.

1. Test-drive the vehicle.