( TL19E00J1616622130AKBAT00 )

Rear Door Outer Molding Replacement

1. While removing the upper edge of the door outer molding (A) from the edge of the sash, cut the double-sided adhesive tape (B) with a utility knife, then remove the molding from the sash. Release the bottom hook (C), then remove the molding.

1. Scrape off the remaining double-sided adhesive tape from the sash, then clean the sash surface with a sponge dampened in isopropyl alcohol.

1. Install the new door outer molding in the reverse order of removal, and note these items:
   - Push the adhesive portions and the bottom hook portion into place securely.
   - Make sure the upper and lower sides of the molding are catching the edges of the sash properly.
   - Push the door weatherstrip clips into place securely.
   - When reinstalling the door panel, make sure the plastic cover is installed properly and sealed around its outside perimeter to seal out water.